Dual-Video Multiplexer Anti-Interference UTP Balun Transceiver Power Type

CCTV Security Camera BNC Anti-interference Video Transmitter/Receiver

Features:

Input voltage: DC 12V

Working current: <=300mA

Output current: 300mA

Video input: 750 ohm 1.0V

Video bandwidth: 10MHz

Power consumption: <10W

Video signal format: NTSC / PAL / CCIR

Transmission distance: 400m~800m

High-frequency interference, low frequency interference and electromagnetic interference, pulse interference, effective solution to image jitter / distortion / blur / color / text grid horizontal text interference, and other function

Video anti-interference device:

It can mainly solve the tough anti-interference problems (including elevators, converting stations, electromotor, industrial converter and various high frequency electromagnetic interference)

It can solve various interferential phenomena such as power frequency, common mode and overlapping curve, etc.

RE602V double video multiplexer:

Video 1 can transmit the distance of 400 meters to 800 meters (and with function of frequency shift type anti-interference device)

Video 2 can transmit 400 meters (used in conjunction with 640T/R of our company, and the transmission distance can reach 1000 meters)

Video UTP balun transceiver:

Long transmission distance and high image quality

Convenient for wiring and high usage of cable

Strong anti-interference ability

Packing List:

1 x Transmitter

1 x Receiver

1 x Power cable (40cm)

1 x English user manual